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FITTINGS
TYPE AND DIMENSIONS OF FITTING


[image: UL Listed Cable Cleats - Power and Cables][image: A picture containing shape

Description automatically generated]
RIGID COUPLING
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	Nominal Size mm/in
	Pipe O.D mm/in
	Working Pressure Bar/KPA
	Bolt Size
	Dimensions mm/in

	
	
	
	No. – Size mm
	ᶲ
	L
	H

	50
2
	60.3
2.374
	20.68
2070
	2-M10*55
	88.4
3.480
	125
4.921
	46
1.732

	65
2 ½
	76.1
3
	20.68
2070
	2-M10*55
	102.2
4.024
	140
5.512
	46
1.772

	80
3
	88.9
3.5
	20.68
2070
	2-M10*60
	117.4
4.622
	154
6.063
	46
1.772

	100
4
	114.3
4.25
	20.68
2070
	2-M12*65
	146.6
5.772
	190
7.480
	48
1.889

	150
6
	165.1
6.5
	20.68
2070
	2-M12*75
	196.2
7.724
	244
9.606
	48
2.008

	200
8
	219.1
8.625
	15.99
1600
	2-M16*85
	256.4
10.024
	326
12.835
	58
2.283

	250
10
	273
10.748
	15.99
1600
	2-M20*100
	316
12.441
	426
16.771
	64
2.520

	300
12
	323.9
12.75
	15.99
1600
	2-M22*130
	380
14.961
	470
18.504
	65
2.559


U-BOLTED MECHANICAL TEE THREADED
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	Nominal Size mm/in
	Pipe O.D mm/in
	Working Pressure Bar/KPA
	Bolt Size
	Dimensions mm/in
	Hole Cutting
Dimensions

	
	
	
	No. – Size mm
	H
	L
	K
	mm/in
+1.6,0/+0.063,0

	25 x 15
1 x 1/2 
	33.7 x 21.3
1.327 x 0.839
	20.68
2070
	M8x25
	43.5
1.713
	74
2.913
	44
1.732
	26
1.024

	32 x 15
1 ¼ x 1/2 
	42.4 x 21.3
1.669 x 0.839
	20.68
2070
	M10x28.5
	47
1.850
	90
2.953
	69
2.717
	30
1.181

	32 x 20
1 ¼ x 3/4 
	42.4 x 26.9
1.669 x 1.059
	20.68
2070
	M10x28.5
	51
2.008
	90
3.543
	56
2.205
	30
1.181

	40 x 15
1 ½ x 1/2 
	48.3 x 21.3
1.900 x 0.839
	20.68
2070
	M10x28.5
	49
1.929
	90
3.543
	56
2.205
	30
1.181

	40 x 20
1 ½ x 3/4
	48.3 x 26.9
1.900 x 1.059
	20.68
2070
	M10x28.5
	53
2.087
	90
3.543
	56
2.205
	30
1.181

	50 x 15
2 x 1/2
	60.3 x 21.3
2.375 x 0.839
	20.68
2070
	M10x30
	56
2.205
	100
3.937
	56
2.205
	30
1.181

	50 x 20
2 x 3/4
	60.3 x 26.9
2.375 x 1.059
	20.68
2070
	M10x30
	60
2.362
	100
3.937
	56
2.205
	30
1.181



FITTINGS
TYPE AND DIMENSIONS OF FITTING


	Nominal Size mm/in
	Pipe O.D mm/in
	Working Pressure Bar/KPA
	Bolt Size
	Dimensions mm/in
	Hole Dia

	
	
	
	No. – Size mm
	ᶲ
	L
	K
	H
	mm/in
+1.6,0/+0.063,0

	80x50
3x2
	88.9x60.3
3.50x2.375
	20.68
2070
	2-M10x60
	113
4.449
	146
5.748
	80.5
3.169
	91
3.583
	61
2.402

	100x80
4x3
	114x88.9
4.50x3.50
	20.68
2070
	2-M12x75
	138
5.433
	176
6.929
	93
3.661
	118
4.545
	86
3.386

	150x100
6x4
	168.3x114.3
6.625x4.50
	20.68
2070
	2-M12x75
	192
7.559
	228
8.976
	120
4.724
	147
5.787
	114
4.488
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MECHANICAL TEE GROOVED
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MECHANICAL TEE THREADED
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	Nominal Size mm/in
	Pipe O.D mm/in
	Working Pressure Bar/KPA
	Bolt Size
	Dimensions mm/in
	Hole Dia

	
	
	
	No. – Size mm
	ᶲ
	L
	K
	H
	mm/in
+1.6,0/+0.063,0

	80x25
3x1
	88.9x33.7
3.500x1.327
	20.68
2070
	2-M10x60
	113
4.449
	146
5.748
	75
2.953
	69
2.717
	38
1.496

	80x50
3x2
	88.9x60.3
3.500x2.375
	20.68
2070
	2-M10x60
	113
4.449
	146
5.748
	75
2.953
	91
3.583
	61
2.402













TYPE AND DIMENSIONS OF FITTING
FITTINGS
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90 ° ELBOW
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	Nominal Size mm/in
	Pipe O.D mm/in
	Working Pressure Bar/KPA
	L mm/in

	
	
	
	Short

	50
2
	60.3
2.375
	20.68
2070
	70
2.756

	65
2 ½
	76.1
3
	20.68
2070
	76
2.992

	80
3
	88.9
3.5
	20.68
2070
	90
3.543

	100
4
	114.3
4.5
	20.68
2070
	102
4.016

	150
6
	165.1
6.5
	20.68
2070
	140
5.512

	200
8
	219.1
8.625
	20.68
2070
	175
6.890

	250
10
	273
10.75
	20.68
2070
	215
8.465














	Nominal Size mm/in
	Pipe O.D mm/in
	Working Pressure Bar/KPA
	L mm/in

	
	
	
	Standard

	50
2
	60.3
2.375
	20.68
2070
	83
3.27

	65
2 ½
	76.1
3
	20.68
2070
	95
3.74

	80
3
	88.9
3.5
	20.68
2070
	108
4.25

	100
4
	114.3
4.5
	20.68
2070
	127
5.00

	150
6
	165.1
6.5
	20.68
2070
	165
6.50

	200
8
	219.1
8.625
	20.68
2070
	197
7.75

	250
10
	273
10.75
	20.68
2070
	229
9.00


















TYPE AND DIMENSIONS OF FITTING
FITTINGS
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45 ° ELBOW
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	Nominal Size mm/in
	Pipe O.D mm/in
	Working Pressure Bar/KPA
	L mm/in

	65
2 ½
	76.1
3
	20.68
2070
	57
2.244

	80
3
	88.9
3.5
	20.68
2070
	64
2.52

	100
4
	114.3
4.5
	20.68
2070
	76
2.992

	150
6
	165.1
6.5
	20.68
2070
	89
3.504

	200
8
	219.1
8.625
	15.99
1600
	108
4.252

	250
10
	273
10.75
	15.99
1600
	121
4.764















CONCENTRIC REDUCER


	Nominal Size mm/in
	Pipe O.D mm/in
	Working Pressure Bar/KPA
	L mm/in

	65x50
2 ½ x 2
	76.1x60.3
2.996x2.375
	20.68
2070
	64
2.62

	80x65
3x2 ½ 
	88.9x76.1
3.5x2.996
	20.68
2070
	64
2.52

	100x80
4x3
	114.3x88.9
1.5x3.5
	20.68
2070
	76
2.992

	150x100
6x4
	168.3x114.3
6.614x4.5
	20.68
2070
	102
4.016

	200x150
8x6
	219.1x165.1
8.626x6.5
	15.99
1600
	127
5
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TYPE AND DIMENSIONS OF FITTING
FITTINGS
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EQUAL TEE
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	Nominal Size mm/in
	Pipe O.D mm/in
	Working Pressure Bar/KPA
	L mm/in

	
	
	
	Short

	50
2
	60.3
2.375
	20.68
2070
	70
2.756

	65
2 ½
	76.1
3
	20.68
2070
	76
2.992

	80
3
	88.9
3.5
	20.68
2070
	86
3.386

	100
4
	114.3
4.5
	20.68
2070
	102
4.016

	150
6
	165.1
6.5
	20.68
2070
	140
5.512

	200
8
	219.1
8.625
	15.99
1600
	175
6.890

	250
10
	273
10.75
	15.99
1600
	215
8.466















	Nominal Size mm/in
	Pipe O.D mm/in
	Working Pressure Bar/KPA
	L mm/in

	
	
	
	Standard

	50
2
	60.3
2.375
	20.68
2070
	83
3.27

	65
2 ½
	76.1
3
	20.68
2070
	95
3.74

	80
3
	88.9
3.5
	20.68
2070
	108
4.25

	100
4
	114.3
4.5
	20.68
2070
	127
5.00

	150
6
	165.1
6.5
	20.68
2070
	165
6.50

	200
8
	219.1
8.625
	15.99
1600
	197
7.75

	250
10
	273
10.75
	15.99
1600
	229
9.00
















TYPE AND DIMENSIONS OF FITTING
FITTINGS
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FLANGE ADAPTOR
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	Nominal Size mm/in
	Pipe O.D mm/in
	Working Pressure Bar/KPA
	Dimensions mm/in
	Bolt/Nut

	
	
	
	Do
	H1
	H2
	ᶲ
	No. – Size mm

	80
3
	88.9
3.5
	15.99
1600
	160
6.299
	17
0.669
	60
2.362
	195
7.677
	8xM16

	100
4
	114.3
4.5
	15.99
1600
	180
7.087
	17
0.669
	60
2.362
	215
8.465
	8xM16

	150
6
	165.1
6.5
	15.99
1600
	240
9.449
	20
0.787
	65
2.559
	280
11.024
	8xM20

	200
8
	219.1
8.625
	15.99
1600
	295
11.614
	20.
0.787
	75
2.952
	330
12.992
	12xM20

	250
10
	273
10.748
	15.99
1600
	295
11.614
	25
0.984
	85
3.346
	400
15.748
	12xM20













REDUCING TEE GROOVED
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	Nominal Size mm/in
	Pipe O.D mm/in
	Working Pressure Bar/KPA
	L mm/in

	100x80
4x3
	108x88.9
4.3x3.5
	20.68
2070
	102
4.016

	150x100
6x4
	165.1x114.3
6.5x4.5
	20.68
2070
	140
5.512














TYPE AND DIMENSIONS OF FITTING
FITTINGS
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CAP
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	Nominal Size mm/in
	Pipe O.D mm/in
	Working Pressure Bar/KPA
	L mm/in

	50
2
	60.3
2.375
	20.68
2070
	26
1.024

	65
2 ½
	76.1
3
	20.68
2070
	28
1.102

	80
3
	88.9
3.5
	20.68
2070
	28
1.102

	100
4
	114.3
4.5
	20.68
2070
	28
1.102

	150
6
	165.1
6.5
	20.68
2070
	28
1.102











RIGID COUPLING GALVANISED
GALVANISED
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	Nominal Size mm/in
	Pipe O.D mm/in
	Working Pressure Bar/KPA
	Bolt Size
	Dimensions mm/in

	
	
	
	No. – Size mm
	ᶲ
	L
	H

	50
2
	60.3
2.374
	20.68
2070
	2-M10*55
	88.4
3.480
	125
4.921
	46
1.732

	65
2 ½
	76.1
3
	20.68
2070
	2-M10*55
	102.2
4.024
	140
5.512
	46
1.772

	80
3
	88.9
3.5
	20.68
2070
	2-M10*60
	117.4
4.622
	154
6.063
	46
1.772

	100
4
	114.3
4.25
	20.68
2070
	2-M12*65
	146.6
5.772
	190
7.480
	48
1.889

	150
6
	165.1
6.5
	20.68
2070
	2-M12*75
	196.2
7.724
	244
9.606
	48
2.008

	200
8
	219.1
8.625
	15.99
1600
	2-M16*85
	256.4
10.024
	326
12.835
	58
2.283

	250
10
	273
10.748
	15.99
1600
	2-M20*100
	316
12.441
	426
16.771
	64
2.520

	300
12
	323.9
12.75
	15.99
1600
	2-M22*130
	380
14.961
	470
18.504
	65
2.559


TYPE AND DIMENSIONS OF FITTING
FITTINGS
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90 ° ELBOW GALVANISED


90 ° ELBOW GALVANISED





	Nominal Size mm/in
	Pipe O.D mm/in
	Working Pressure Bar/KPA
	L mm/in

	
	
	
	Short

	50
2
	60.3
2.375
	20.68
2070
	70
2.756

	65
2 ½
	76.1
3
	20.68
2070
	76
2.992

	80
3
	88.9
3.5
	20.68
2070
	90
3.543

	100
4
	114.3
4.5
	20.68
2070
	102
4.016

	150
6
	165.1
6.5
	20.68
2070
	140
5.512

	200
8
	219.1
8.625
	20.68
2070
	175
6.890

	250
10
	273
10.75
	20.68
2070
	215
8.465
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	Nominal Size mm/in
	Pipe O.D mm/in
	Working Pressure Bar/KPA
	L mm/in

	
	
	
	Standard

	50
2
	60.3
2.375
	20.68
2070
	83
3.27

	65
2 ½
	76.1
3
	20.68
2070
	95
3.74

	80
3
	88.9
3.5
	20.68
2070
	108
4.25

	100
4
	114.3
4.5
	20.68
2070
	127
5.00

	150
6
	165.1
6.5
	20.68
2070
	165
6.50

	200
8
	219.1
8.625
	20.68
2070
	197
7.75

	250
10
	273
10.75
	20.68
2070
	229
9.00
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TYPE AND DIMENSIONS OF FITTING
FITTINGS
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EQUAL TEE GALVANISED
GALVANISED





	Nominal Size mm/in
	Pipe O.D mm/in
	Working Pressure Bar/KPA
	L mm/in

	
	
	
	Short

	50
2
	60.3
2.375
	20.68
2070
	70
2.756

	65
2 ½
	76.1
3
	20.68
2070
	76
2.992

	80
3
	88.9
3.5
	20.68
2070
	86
3.386

	100
4
	114.3
4.5
	20.68
2070
	102
4.016

	150
6
	165.1
6.5
	20.68
2070
	140
5.512

	200
8
	219.1
8.625
	15.99
1600
	175
6.890

	250
10
	273
10.75
	15.99
1600
	215
8.466
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	Nominal Size mm/in
	Pipe O.D mm/in
	Working Pressure Bar/KPA
	L mm/in

	
	
	
	Standard

	50
2
	60.3
2.375
	20.68
2070
	83
3.27

	65
2 ½
	76.1
3
	20.68
2070
	95
3.74

	80
3
	88.9
3.5
	20.68
2070
	108
4.25

	100
4
	114.3
4.5
	20.68
2070
	127
5.00

	150
6
	165.1
6.5
	20.68
2070
	165
6.50

	200
8
	219.1
8.625
	15.99
1600
	197
7.75
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TYPE AND DIMENSIONS OF FITTING
FITTINGS




P CLIPS
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	P Clip Size
mm

	M 8
	M 12











PIPE HANGER
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	Pipe Hanger Size
mm

	25
	32
	40
	50
	65
	80
	100
	150
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Rigid coupling XGQT1

According to different situations, the
appearance can be dealed with epoxy
powder, galvanized, paint,dacromet or
your requirements.
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U-Bolted Mechanical Tee(Threaded) - XGQT3U
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According to different situations, the
appearance can be dealed with epoxy
powder, galvanized, paint,dacromet or
your requirements.
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90° Elbow - XGQTO1
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45° Elbow - XGQTO02
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Equal Tee - XGQTO03
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According to different situations, the appearance can be dealed with epoxy powder, galvanized,
paint,dacromet or your requirements.
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